**Vibox Serial Connection**

To establish a serial connection, the following “usb to serial adapter” can be used.

Example:



The above cable has a subD9 on one side. The following image shows the Pin Layout of the RS232.



And a M12 8 pin connector having the pin1 and 2 connected and ground (pin5)





Once the connections are established through the CAN/Serial Port as per the above information. To access the Vibox now, the following steps must be followed:

Software Used:Putty

Mode of connection: Serial

Serial Line: COM port of the laptop where the USB is connected.

SPEED: 115200

Example when using a COM8 Port.



For the above, to know which port to use, check the device Manager >> Ports (COM & LPT)