# **Vib360 software update in vibox using vibacq**

# **Purpose of the document**

The present document explain the procedure to update the embedded Vibox from Vibacq and a installation package “**installVib360.tar.gz**”

# **Update the embeded box « Vibox » using Vibacq**


Prerequisite:


* PC with Vibacq software installaed
* The Vibox to update connected to the PC via an ethernet/internet connection

1. Start Vibacq
2. Check that you are “Admin” you should see “AdminMode” in the third menu:



* 1. If not click on “UserMode” menu and hit “vib360” as password






* 1. click OK and we are now in “AdminMode”:




1. click on the « **Hardware** » menu




* 1. click on the « **Config** » button




1. Click on « **UpdateSoftware** » button:



1. Browse to the directory where the package **installVib360.tar.gz**  is located. Exemple:



1. Select the file and click on the « Open » button. After a couple of seconds you should see the following message « Update Sent » appearing in green in the upper left of the screen:



* After around 1 minutes the Vibox will be updated

# **VérifY the Vibox Mac adress**


Prerequisite:

* PC with Vibacq software installaed
* The Vibox to update connected to the PC via an ethernet/internet connection

1. Brancher le PC à la Vibox
2. Démarrer Vibacq
   1. Click on menu « Hardware » :



* 1. Select the correct IP of the Vibox (for exemple 192.168.99.11)



* 1. The MAC adress and vesion is visible there  :

